



Monitor Enable jumper open, factory configuration



EXTCTRL jumper, was Hi for +24VDC RF enable, now LOW for 5VDC Oxford 100 direct control 05/12/2016



Main board



JP2 factory configuration, function ?